#!/bin/sh       

NEODEVICE=`cat /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/.location`
IMAGEKATALOG=ImageBoot
UPLOADKATALOG=ImagesUpload

TARGET=Flash
if [ -f $NEODEVICE$IMAGEKATALOG/.neonextboot ]; then
	  TARGET=`cat $NEODEVICE$IMAGEKATALOG/.neonextboot`
fi

if [ ! -e  $NEODEVICE$IMAGEKATALOG/.neonextboot ]; then
	            mnttest="nouuid"
	            if [ -e $NEOBOOT/bin/install  ]; then
    	                orgimag1=`mount | sed '/sd/!d' | cut -d" " -f1`
		        selectinstall=`cat $NEOBOOT/bin/install`
		        for item in $orgimag1; do
			        selectmnt=`blkid | sed "/$selectinstall/!d" | cut -d":" -f1`
			        if [ $selectmnt == $item ]; then
				        echo "selectmnt=" $selectmnt
                        	        mnttest="uuid"
				        mount $selectmnt $NEODEVICE > /dev/null 2>&1
			        fi
			        if [ ! -e $NEODEVICE$IMAGEKATALOG  ]; then
				        echo "NEOBOOT hasn't been installed on: " $selectmnt
				        umount $NEODEVICE > /dev/null 2>&1 
			        else
				        echo "NEOBOOT has been installed on: " $selectmnt
				        break;
			        fi 			
		        done
	            fi
fi

if [ ! -e $NEODEVICE$IMAGEKATALOG/.neonextboot ] ; then 
    export PATH=/bin:/usr/bin:/sbin:/usr/sbin
    /bin/mount -t proc proc /proc > /dev/null 2>&1
    /bin/mount -t sysfs sysfs /sys > /dev/null 2>&1
    /sbin/depmod -Ae > /dev/null 2>&1  
    /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/files/mountpoint.sh 
fi

if [ ! -e  $NEODEVICE$IMAGEKATALOG/.neonextboot ]; then
          ln -sfn /sbin/init.sysvinit /sbin/init
          echo "Flash " > $NEODEVICE$IMAGEKATALOG/.neonextboot
          echo "Error - Back to Flash... "
          sleep 5; #reboot -f
fi 


if [ $TARGET = "Flash" ]; then
		echo "BOOTNEO is booting image from " $TARGET 
		/usr/bin/showiframe /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/neowait.mvi > /dev/null 2>&1
    sleep 3		
		ln -sfn /sbin/init.sysvinit /sbin/init
		#reboot -f
else
    ######### test boot new imaga>>>>
    VUMODEL=$( cat /proc/stb/info/vumodel )
    BOXNAME=$( cat /etc/hostname)
    DIRECTORY=ImageBoot
    UPLOAD=ImagesUpload	
    DEVICEBOOT=`cat /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/.location`
    if [ -e $DEVICEBOOT$DIRECTORY/$TARGET/.control_ok ]; then
        [ $PL ] && echo "Nie ma bledu, normalny start image..." || echo "No Error - Booting image normal..."
    elif [ -e $DEVICEBOOT$DIRECTORY/$TARGET/.control_boot_new_image ]; then
        echo "First start image - The first attempt to launch a new image... "; rm -f $DEVICEBOOT$DIRECTORY/$TARGET/.control_boot_new_image 
    else        
	      if [ -f `cat /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/.location`$IMAGEKATALOG/$TARGET/boot/zImage.$BOXNAME ]; then
            VUMODEL=`cat /proc/stb/info/vumodel` 
            BOXNAME=`cat /etc/hostname`
            if [ ! -e $DEVICEBOOT$DIRECTORY/$TARGET/.control_ok ] ; then                                          
                if [ $BOXNAME = "vuultimo4k" ] || [ $BOXNAME = "vusolo4k" ] || [ $BOXNAME = "vuuno4kse" ] || [ $BOXNAME = "vuuno4k" ]; then                                                         			        
                    if [ -d /proc/stb ] ; then
                        echo " Install kernel image flash.... " $BOXNAME
                        dd if=$DEVICEBOOT$UPLOAD/.kernel/flash-kernel-$VUMODEL.bin of=/dev/mmcblk0p1
                    fi
                elif [ $BOXNAME = "vuzero4k" ] ; then                                                         			        
                    if [ -d /proc/stb ] ; then
                        echo " Install kernel image flash.... " $BOXNAME
                        dd if=$DEVICEBOOT$UPLOAD/.kernel/flash-kernel-$VUMODEL.bin of=/dev/mmcblk0p4
                    fi
                elif [ $BOXNAME = "vuduo4k" ] ; then                                                         			        
                    if [ -d /proc/stb ] ; then
                        echo " Install kernel image flash.... " $BOXNAME
                        dd if=$DEVICEBOOT$UPLOAD/.kernel/flash-kernel-$VUMODEL.bin of=/dev/mmcblk0p6
                    fi
                fi                                            
            fi
        fi    
        /usr/bin/showiframe /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/error.mvi > /dev/null 2>&1
        echo "Wrong kernel. Press number 3"  > $DEVICEBOOT$UPLOAD/.kernel/used_flash_kernel
        ln -sfn /sbin/init.sysvinit /sbin/init
        echo "Flash "  > $DEVICEBOOT$DIRECTORY/.neonextboot
 			  echo "Error - NeoBoot he can not run it image !!! "
 			  echo "Restart STB - Back to Flash... "
  		  sleep 10; #reboot -f   
    fi

    ######### test boot new image<<<<<
    if [ -e $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh ] ; then
        rm -f $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh 
    fi
    cp -f /usr/lib/enigma2/python/Plugins/Extensions/NeoBoot/files/mountpoint.sh $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh

    #mount $NEODEVICE /media/neoboot 
    if [ -e $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh ] ; then
                                orgimag=`mount | sed '/sd/!d' | cut -d" " -f1`
                                   for item in $orgimag; do
                                       ohdd=`echo  $item | cut -d"/" -f3`
                                       nhdd=`mount | sed "/\$ohdd/!d" | sed q | cut -d" " -f3`
                                       if [ $nhdd == '/media/usb' ]  ; then
                                          echo $nhdd
                                          echo "mkdir "$nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh
                                          echo "mount "$item $nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh 
                                          echo "[NeoBOOT] created in /usr/bin the file enigma2_pre_start.sh "
                                       elif [ $nhdd == '/media/hdd' ] ; then
                                          echo $nhdd
                                          echo "mkdir "$nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh
                                          echo "mount "$item $nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh 
                                          echo "[NeoBOOT] created in /usr/bin the file enigma2_pre_start.sh "
                                       else
                                          echo "umount "$nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh
                                          echo "mkdir "$nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh
                                          echo "mount "$item $nhdd  >> $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh 
                                          echo "[NeoBOOT] enigma2_pre_start.sh "
                                          echo ok 
                                       fi    
                                   done                             
    fi                            
    chmod 0755 $NEODEVICE$IMAGEKATALOG/$TARGET/usr/bin/enigma2_pre_start.sh 
    echo "NeoBOOT created the file mount enigma2_pre_start.sh "
    sleep 2 
fi
                                   
exit 0
        